Booster Pump
Permanent Magnet Variable Frequency Booster Pump
Our permanent magnet variable frequency booster pump operates a safe voltage of 24-48v running very silent at 30dB always giving you clean water without rust as cheaper traditional pumps will give you. The High-Efficiency Permanent Magnet Motor: Ensures maximum energy savings and smooth operation. It has a easy to use interface to set pump flow.

Product details
APPLICATION
· Well water lifting and water tower water filling
· Living water supply and garden irrigation
· Pipeline pressure boosting and supporting equipment (solar energy water supply system, water heater, etc.）
· Transfer clean water or non-corrosive liquid without solid particles and fibers
WORKING CONDITION
	Liquid temperature
	0 - 100℃

	Ambient temperature
	4 - 55℃

	Max. suction
	+9m

	Insulation
	ClassH

	Waterproof rating
	IP55

	Duty cycle
	S1

	Input voltage
	Single phase
100-140V, 50/60Hz
160-240V, 50/60Hz


MODEL INSTRUCTION
	25ZPZ/24V/B/H20-Q2.0

	25: Inlet&outlet diameter (mm)

	ZPZ: Intelligent permanent magnet canned booster pump

	24V: DC - 24V

	B: Product series

	H20：Max. head 20m

	Q2.0：Max. flow 2.0m³/h


TECHNICAL PARAMETER  (n=12000r/min)
	 Model
	Voltage
（V）
	Power
(W)
	Power
(HP)
	Max. flow
（m³/h）
	Max. flow
（l/min）
	Max. head
（m）
	Max. suction
（m）
	Inlet&Outlet
(inch)

	25ZPZ/24V/B/H20-Q2.0
	DC-24
	84
	0.1
	2.0
	33
	20
	9
	1"×1"

	25ZPZ/30V/B/H25-Q2.2
	DC-30
	105
	0.1
	2.2
	37
	25
	9
	1"×1"

	25ZPZ/36V/B/H30-Q2.4
	DC-36
	126
	0.2
	2.4
	40
	30
	9
	1"×1"

	25ZPZ/40V/B/H35-Q2.5
	DC-40
	160
	0.2
	2.5
	42
	35
	9
	1"×1"




